In the current shape, the pcb measures 230 mm x 115 mm.  
With the FPGA the footprint will increase to 230 x 192 mm.

Vertically we need ~ 35 mm + any spacer.  
  
http://uk.rs-online.com/web/p/instrument-cases/0222115/  
  
http://uk.rs-online.com/web/p/instrument-cases/7545995/  
  
http://uk.rs-online.com/web/p/instrument-cases/0232002/

http://uk.rs-online.com/web/p/instrument-cases/8673303/